Step1:

Install PC software—>Open Client.exe(Initialization must be successful and connect server)—>Send command as \*IDN? , \*ADC?CH1 , \*RDM? etc.

tips:

The commands reference <<PC Series SCPI Protocol V1.3.docx>>;

Step2 : Set SCPI port (the port is 5188 as default).



Step3: Write software that belongs to you, you coule reference the source code of Client.exe